# Check Valves

CRANE Duo-check high-performance check valves and wafer-type check valves to prevent backflow. Disc and swing type for various applications. 50–600 mm.

CRANE Duo-Check

## High Performance Check Valves

CRANE Duo-Check high-performance dual plate wafer check valves. Compact design with minimal pressure drop. Suitable for water, steam, gas and oil services.

Size | 50 mm to 600 mm
Body | CI / WCB / SS
Disc | WCB / SS / Al. Bronze
Seat | Rubber / Metal Seated
Type | Dual Plate Wafer
Standards | API 594, API 598
Brand | CRANE

Wafer Check

## Wafer Check Valves

Economical wafer-type check valves for standard services. Low pressure drop design. Available in rubber and metal seated options.

Size | 50 mm to 600 mm
Body | CI / WCB / SS
Type | Wafer / Swing
Seat | Rubber / Metal
Brand | CRANE

### Need a quote for Check Valves?

Our technical team will respond with the best solution and pricing.

Send Enquiry 📞 98422 24050
💬