# Gate / Globe / NRV Valves

Cast and forged steel gate, globe and non-return valves from CRANE. For high-pressure and high-temperature applications across all process industries. 15–600 mm, Class 150–1500.

CRANE Gate Valves

## Gate Valves

Full bore gate valves for on/off isolation service. Minimal pressure drop in the open position. Suitable for steam, water, oil and gas services.

Size | 15 mm to 600 mm
Body | WCB / SS / Hastelloy / Monel
Wedge | WCB / SS / Hastelloy / Monel
Rating | Class 150 / 300 / 600 / 800 / 1500
Ends | Screwed / Socket Weld / Flanged
Operation | Handwheel / Worm Gear / Pneumatic / Electric
Brand | CRANE

CRANE Globe Valves

## Globe Valves

Globe valves for throttling and flow regulation. Good shutoff capability and suitable for frequent operation. Available in various trim materials.

Size | 15 mm to 600 mm
Body | WCB / SS / Hastelloy / Monel
Rating | Class 150 / 300 / 600 / 800 / 1500
Ends | Screwed / Flanged / Butt Weld
Operation | Handwheel / Gear / Pneumatic / Electric
Brand | CRANE

CRANE Non-Return Valves

## Non-Return / Check Valves

Swing check and duo-check non-return valves to prevent backflow. Suitable for water, steam and process gas applications.

Size | 15 mm to 600 mm
Body | WCB / SS / Hastelloy / Monel
Rating | Class 150 / 300 / 600 / 800 / 1500
Type | Swing / Duo-Check
Brand | CRANE

### Need a quote for Gate / Globe / NRV Valves?

Our technical team will respond with the best solution and pricing.

Send Enquiry 📞 98422 24050
💬