# Piston Valves

High-quality piston valves for accurate flow control in process systems. Available in WCB, SS, Hastelloy and Monel for various process fluids. 15–300 mm.

Pennant Piston Valves

## Piston Valves

Precision piston valves providing accurate flow control. The piston design ensures tight shutoff and long service life.

Size | 15 mm to 300 mm
Body | WCB / SS / Hastelloy / Monel
Wedge | WCB / SS / Hastelloy / Monel
Rating | Class 150 / 300 / 600 / 800
Ends | Screwed / Socket Weld / Flanged
Operation | Handwheel / Worm Gear / Pneumatic / Electric
Brand | Pennant

Saunders Angle Seated

## Angle Seated Piston Valves

Crane Saunders angle-seated piston valves for high-flow, fast-acting service. Ideal for steam, water and compressed air systems.

Size | 15 mm to 65 mm
Body & Internals | SS 304 / SS 316 / SS 316L
Seat | PTFE / CFT / GFP / PEEK / Delrin
Ends | Screwed / Flanged / Triclover
Operation | Manual / Pneumatic Actuators
Brand | Saunders

### Need a quote for Piston Valves?

Our technical team will respond with the best solution and pricing.

Send Enquiry 📞 98422 24050
💬