# Our Product Range

A comprehensive range of industrial valves, actuators and instruments from CRANE, Saunders, ARI Armaturen and more — for every process industry requirement.

Complete Range Available

## Total Flow Solutions Under One Roof

From small bore manual valves to large actuated butterfly valves, from pharma-grade diaphragm valves to heavy-duty gate valves — we stock it all.

Request a Quote ›

### Butterfly Valves

Manual, actuated and high-performance butterfly valves. Wafer, lug and flanged body types. Suitable for water, slurry, chemical and food applications.

40–1200 mm CI / WCB / SS EPDM / NITRILE / TEFLON CRANE
View Details ›

### Diaphragm Valves

Industrial and aseptic pharma-grade diaphragm valves by Saunders. Ideal for hygienic, sterile and corrosive fluid applications.

15–350 mm CI / WCB / SS Rubber / PTFE Saunders
View Details ›

### Ball Valves

Floating and trunnion mounted ball valves. 2-piece, 3-piece and flanged configurations. Full bore and reduced bore options.

15–300 mm WCB / SS / Hastelloy Class 150–800 CRANE
View Details ›

### Gate / Globe / NRV Valves

Cast and forged steel gate, globe and non-return valves for high-pressure and high-temperature services across all process industries.

15–600 mm WCB / SS / Hastelloy Class 150–1500 CRANE
View Details ›

### Control Valves

ARI Armaturen diaphragm-operated globe control valves, thermic fluid bellow seal globe valves and pressure reducing valves.

25–200 mm WCB / SS Pneumatic / Motorised ARI Armaturen
View Details ›

### Lined Valves

PFA, PTFE, PVDF and PP lined ball and butterfly valves for handling highly corrosive chemicals and aggressive media.

15–300 mm PFA / PTFE / PVDF / PP Class 150 & 300 CRANE
View Details ›

### Check Valves

Duo-check high-performance and wafer-type check valves. Disc and swing type for preventing backflow in pipelines.

50–600 mm CI / WCB / SS Rubber / Metal Seated CRANE
View Details ›

### Piston Valves

Precision piston valves for accurate flow control. Available in WCB, SS, Hastelloy and Monel for various process fluids.

15–300 mm WCB / SS / Hastelloy Class 150–800 Pennant
View Details ›

### Steam Traps

Ball float and thermodynamic steam traps for efficient condensate removal in steam systems. CI, WCB and SS body.

15–100 mm CI / WCB / SS Ball Float / TD Pennant
View Details ›

### Actuators & Accessories

REVO quarter-turn pneumatic actuators (double-acting and spring-return), solenoid valves, positioners and limit switches.

DA & SR NAMUR / ISO REVO / Saunders
View Details ›

### Instruments & Spares

Pressure gauges, positioners, limit switches, solenoid valves, knife gate valves, spare teflon seats and diaphragms.

Various Sizes Multiple Brands
View Details ›
💬