# Ball Valves

Full-bore and reduced-bore ball valves from CRANE. Available in WCB, SS, Hastelloy and Monel for demanding process applications. 15–300 mm, Class 150–800.

Manual Ball Valves

## Flanged & Screwed Ball Valves

High-quality two-piece and three-piece ball valves in SS 304/316 and WCB. Full bore design for minimum pressure drop.

Size | 15 mm to 300 mm
Body | WCB / SS / Hastelloy / Monel
Ball & Stem | SS 304 / SS 316 / Hastelloy
Rating | Class 150 / 300 / 600 / 800
Seat | PTFE / Delrin / PEEK / Metal Seated
Ends | Screwed / Socket Weld / Flanged
Brand | CRANE

2-Piece & 3-Piece

## Multi-Piece Ball Valves

2-piece and 3-piece SS ball valves. The 3-piece design allows for in-line maintenance without removing the valve from the pipeline.

Sizes | 15 mm to 100 mm
Construction | 2-piece / 3-piece
Material | SS 304 / SS 316
Ends | Screwed / Flanged / Weld
Rating | Class 150–2500

Pneumatic & Motorised

## Actuated Ball Valves

Pneumatically actuated and motorised ball valves for automated on/off and modulating control. Available in screwed and flanged ends.

Size | 15 mm to 300 mm
Body | WCB / SS
Actuator | Pneumatic / Electric Motor
Operation | Double Acting / Spring Return
Accessories | SOV + Limit Switch + Positioner

High-Pressure Flanged

## Flanged Actuated Ball Valves

Large-bore flanged ball valves with pneumatic or electric actuators for high-pressure pipeline automation. CI and SS body options.

Size | 25 mm to 300 mm
Body | CI / WCB / SS
Flanges | PN 10/16, ANSI 150/300
Actuator | Pneumatic / Electric

### Need a quote for Ball Valves?

Send us your requirements and our technical team will respond with the best solution and pricing.

Send Enquiry 📞 98422 24050
💬