# Butterfly Valves

Manual, actuated and high-performance butterfly valves from CRANE. Wafer, lug and flanged types for water, chemical, slurry and food industries. DN 40–1400.

CRANE Manual Butterfly Valves

## Manual Butterfly Valves

Resilient seated butterfly valves designed for tight shutoff in abrasive and corrosive environments. Only 2 wetted parts for maximum corrosion resistance.

Size | 40 mm to 1200 mm
Body | CI / WCB / SS
Disc | SGI / SS / Teflon Coated
Seat | EPDM / Nitrile / Teflon
Operation | Manual Lever / Gear
Standard | EN 593, API 609, ISO 5211
Brand | CRANE Center Line RS

CRANE Actuated Butterfly Valves

## Actuated Butterfly Valves

Pneumatically and motorised actuated butterfly valves for automated process control. Suitable for open/close and modulating service.

Size | 40 mm to 1200 mm
Body | CI / WCB / SS
Disc | SGI / SS / Teflon Coated
Seat | EPDM / Nitrile / Teflon
Operation | Pneumatic / Motorised
Brand | CRANE Center Line RS

CRANE High Performance

## High Performance Butterfly Valves

Double-offset or triple-offset design for tight shutoff at higher pressures and temperatures. Metal seated for extreme service conditions.

Size | 40 mm to 600 mm
Body | WCB / SS
Disc | WCB / SS
Seat | RTEF / Metal Seated
Operation | Manual / Worm Gear / Pneumatic / Motorised
Brand | CRANE Flowseal

### Need a quote for Butterfly Valves?

Send us your requirements and our technical team will respond with the best solution and pricing.

Send Enquiry 📞 98422 24050
💬