# Lined Valves

PFA, PTFE, PVDF and PP lined ball and butterfly valves from CRANE for handling highly corrosive acids, alkalis and aggressive chemicals. 15–300 mm, Class 150 & 300.

CRANE Lined Ball Valves

## Lined Ball Valves

Fully lined ball valves for corrosive service. Body and ball/stem lined with PFA, PTFE, PVDF or PP for complete chemical resistance.

Size | 15 mm to 300 mm
Body Lined | PFA / PTFE / PVDF / PP
Ball & Stem | Lined with PFA / PTFE / PVDF / PP
Rating | Class 150 / 300
Seat | PTFE / Delrin / PEEK
Operation | Manual / Pneumatic / Electric Actuators
Brand | CRANE

Applications

## Ideal for Corrosive Media

Lined valves are the go-to solution when the process fluid would attack conventional metal valves. The lining protects the valve body entirely from the media.

#### Hydrochloric Acid (HCl)

PFA and PTFE linings provide excellent resistance to HCl at all concentrations.

#### Sulphuric Acid & Caustic Soda

PVDF and PP linings handle these common industrial chemicals effectively.

### Need a quote for Lined Valves?

Our technical team will respond with the best solution and pricing.

Send Enquiry 📞 98422 24050
💬