# Electric Actuators

Multi-Turn & Quarter-Turn

## Electric Valve Actuators

Fluidcare supplies multi-turn and quarter-turn electric actuators for remote valve automation where instrument air is not available or is undesirable. Suitable for on/off open-close duty, modulating (positioning) duty, and regulating applications.

Our electric actuator range includes integral controls with local/remote operation, adjustable torque and position limits, visual position indication and 4–20mA feedback signal as standard. Available in standard, explosion-proof (ATEX) and weatherproof enclosures.

- Multi-turn and quarter-turn configurations
- On/off and modulating (4–20mA) duty versions
- Integral controls with local/remote switching
- 4–20mA position feedback as standard
- ATEX certified explosion-proof options available
- ISO 5211 mounting — compatible with all valve types

Actuator Type | Multi-Turn (MT), Quarter-Turn (QT)
Output Torque | 10 Nm to 32,000 Nm (multi-turn)
Power Supply | 24VDC, 110VAC, 230VAC, 415VAC 3-Phase
Control Signal | Open/Close (digital), 4–20mA modulating
Feedback | 4–20mA, 0–10V, Limit Switches (2 or 4)
Enclosure | IP67, IP68; ATEX Zone 1/21, Zone 2/22
Standards | IEC 60034, EN 50014, ATEX 94/9/EC

Remote Locations Water Treatment HVAC Systems Power Generation Building Services Chemical Plants
Request a Quote All Products

## No Instrument Air? No Problem.

Our electric actuator range gives you full remote control and automation capability without compressed air infrastructure.

Enquire Now View All Products