# Control Valves

Globe Style — Pneumatic & Electric

## Process Control Valves

Fluidcare supplies globe style control valves with pneumatic and electric actuators for precise flow, pressure and temperature regulation. Available with digital positioners, limit switches, solenoid valves and a full range of accessories for integration into modern DCS and SCADA systems.

Our control valve range is sized to your specific process conditions using recognised flow equations including Cv/Kv calculation, with full documentation packages available including CV calculations, material certificates and test reports.

- Globe single-seated and double-seated designs
- Digital HART positioners for precise control
- Equal percentage, linear and quick-open trim
- Full port and reduced port options
- Caged trim for high pressure drop service
- 3-way mixing and diverting configurations

Size Range | DN 15 – 300 (½" – 12")
Pressure Rating | ANSI 150–2500 / PN 10–400
Temperature | -200°C to +450°C
Body Style | Globe, Angle, 3-Way
Body Material | Carbon Steel, SS 304/316, Alloy Steel
Actuator | Pneumatic Spring-Diaphragm, Electric
Standards | IEC 60534, ISA S75, ANSI FCI 70-2

Oil & Gas Power Generation Chemical Refining Pulp & Paper HVAC Systems
Request a Quote All Products

## Need Cv Calculations?

Our engineers can perform full sizing calculations for your control valve application and provide complete specification documentation.

Talk to an Engineer View All Products