# Ball Valves

Full Bore & Reduced Bore

## Industrial Ball Valves

A comprehensive range of industrial ball valves designed for reliable on/off and throttling service. Available in 2-piece and 3-piece body construction with screwed or flanged end connections in stainless steel, carbon steel and cast iron.

Available with manual lever handles or fully automated with pneumatic or electric actuators. All valves are manufactured to API 6D, API 608, and ASME B16.34 standards.

- Full bore and reduced bore for maximum flow efficiency
- 2-piece and 3-piece body for easy in-line maintenance
- Anti-blowout stem design — operational safety
- PTFE-reinforced seats for chemical resistance
- ISO 5211 direct actuator mounting interface
- Lockable lever handle as standard on manual versions

Size Range | DN 15 – 300 (½" – 12")
Pressure Rating | PN 10–40 / ANSI 150–600
Temperature | -29°C to +200°C
End Connections | Flanged (EN 1092 / ANSI B16.5), Screwed NPT/BSP
Body Material | Carbon Steel, SS CF8M/CF3M, Cast Iron
Seat Material | PTFE, Reinforced PTFE, PEEK
Standards | API 6D, API 608, ASME B16.34, EN 1983

Oil & Gas Petrochemical Chemical Processing Water Treatment Power Generation Pharmaceutical
Request a Quote All Products

## Get a Competitive Quote.

Our technical team will help you select the right ball valve specification for your pressure, temperature and media requirements.

Contact Our Team View All Products