# Control Valves

ARI Armaturen diaphragm-operated globe control valves, thermic fluid bellow seal globe valves, and pressure reducing valves. Pneumatic and motorised operation.

ARI Armaturen

## Diaphragm Operated Globe Control Valves

Precision control valves with pneumatic diaphragm actuators for accurate flow, pressure and temperature control in process plants.

Size | 25 mm to 200 mm
Type | Two Way & Three Way
Body | WCB / SS
Internals | SS
Operation | Pneumatic Diaphragm Actuated / Motorised
Accessories | E/P Positioner + AFR + SOV + Tubing
Brand | ARI Armaturen

ARI Armaturen

## Thermic Fluid Bellow Seal Globe Valves

Zero-leakage bellow seal globe valves specifically designed for thermic fluid and hot oil services. Prevents fugitive emissions.

Size | 25 mm to 200 mm
Type | Two Way & Three Way
Body | WCB / SS
Seal | Bellow Seal, Zero Leakage
Operation | Pneumatic Diaphragm Actuated / Motorised
Accessories | E/P Positioner + AFR + SOV + Tubing
Brand | ARI Armaturen

ARI Armaturen

## Pressure Reducing Valves

Self-operated pressure reducing valves for maintaining downstream pressure at a set value. No external energy required.

Size | 25 mm to 200 mm
Body | WCB / SS
Internals | SS
Operation | Pneumatic Diaphragm Actuated
Set Pressure | Adjustable
Brand | ARI Armaturen

### Need a quote for Control Valves?

Our technical team will respond with the best solution and pricing.

Send Enquiry 📞 98422 24050
💬