# Steam Traps

Ball float and thermodynamic steam traps from Pennant for efficient condensate removal. CI, WCB and SS body. 15–100 mm.

Pennant Steam Traps

## Ball Float & Thermodynamic Steam Traps

Reliable steam traps for condensate drainage in steam distribution systems. Ball float type for continuous drainage, thermodynamic for intermittent drainage.

Size | 15 mm to 100 mm
Body | CI / WCB / SS
Internals | SS304 / SS316
Ends | Screwed / Socket Weld / Flanged
Type | Ball Float / Thermodynamic
Brand | Pennant

#### Why Good Steam Traps Matter

Inefficient steam traps lead to energy waste, water hammer, and equipment damage. Properly sized traps improve system efficiency and reduce operating costs.

### Need a quote for Steam Traps?

Our technical team will respond with the best solution and pricing.

Send Enquiry 📞 98422 24050
💬