# Our Products

Valves

## Industrial Valve Range

Precision-engineered valves for every process condition — from clean water to aggressive chemicals, abrasive slurries and aseptic pharmaceutical applications.

### Butterfly Valves

Center Line® Series RS resilient seated butterfly valves. DN 40–1400. PN 10–16, ANSI 150. Wafer, lug and flanged body types. ISO 9001 certified, PED/FDA approved.

View Details

### Ball Valves

Full bore and reduced bore ball valves. 2-piece and 3-piece construction. Flanged and screwed ends. Stainless steel, carbon steel and cast iron. ANSI 150–600.

View Details

### Control Valves

Globe style pneumatic and electric control valves with positioners for precise flow regulation. Suitable for pressure, temperature and flow control applications.

View Details

### Diaphragm Valves

Saunders A Type (weir) and KB Type (straight-through) diaphragm valves. ¼" to 14". Cast iron, stainless steel, bronze. For abrasive, corrosive and aseptic applications.

View Details
Actuators

## Actuator Range

Complete automation solutions from simple on/off operation to precise modulating control, with full accessory integration.

### Pneumatic Actuators

REVO quarter-turn rack and pinion actuators. Double-acting (RD series) and single-acting spring-return (RS/A series). 2.2 Nm to 11,752 Nm. ISO/NAMUR interfaces.

View Details

### Electric Actuators

Multi-turn and quarter-turn electric actuators for remote valve operation. Suitable for modulating, open/close and positioning duty. With integral limit switches and position feedback.

View Details

## Can't Find What You Need?

Our engineering team can source specialised valves and actuators to meet your exact process requirements. Contact us for a consultation.

Contact Our Engineers